GUIDE TECHNOLOGY(HK) LIMITED

INSTALLATION MANUAL

Car Model: YL-6314 Nissan Paladin 2023+

Installation Requirement Safety Precautions

For your safety and normal using, please ask a professional personal to install it, do not install and uninstall by yourself, to avoid product damage or accidents.

Before installation, please make sure car mfd showing normally, all buttons inside car are working correctly, check if car light working, if have some scratches inside car surface, if yes, please contact with car owner.

Check if tailgate open and close normally, if has any deformations.

Prepare all tools, turn off car, ensure power off operation.

5.The parts and screws of the original car removed during installation should be placed separately and marked to prevent loss. Wire joints should be insulated to prevent short circuit.

6.According to the wiring mode of our company, avoid affecting the moving parts of the car when installation, such as steering wheel drive shaft, accelerator and brake pedal and other vehicle control parts. The wiring harness should be fixed during the straight line process to prevent loose.

7.Do not plug in or out the product and plug in the power-on state, to avoid damage to the product.

Step1: Wirring definition.

Pole serial no. seventh-bottom “L” means left pole, “R” means right pole, “G” means no need recognize.

Installation process diagram

Note: The installation step is to install the mechanical part of the pole firstly, open and close tailgate manually, and confirm that the polo open and close smoothly and the polo body does not scratch the car body, then connect the power and signal, then test again, if not problem, we can finish wiring followed our installation requirements.

Connect control box.

Rear button connector.

Connect our 3-ways connector.

Connect our suction lock(green color unlock signal, orange second lock signal).

Connect our power cable white color, its for kick sensor.

Kick sensor signal connector. Without kick sensor no need connect.

Kick sensor connector. Without kick sensor no need connect.

Control box power connector.

Battery.

ACC.

GND.

Second lock signal.

Rear button signal.

Rear button light.

Reserved.

CAN-L.

Unlock signal.

Rear button GND.

B-pillar unlock signal.

Manual signal.

CAN-H.

Above positions are the wiring diagrams of some models.

NOTE：After installed pole and lock, please open and close door manually to make sure it working perfectly without any scrub, then connect cable and testing with power on again, if working perfect, then we can begin to make wiring.

Take off this 2 snaps and original handle frame, then take off decoration frame.

Take off original hydraulic pressure rod.

Take off original bracket.

Install our special bracket.

Install our electric rod.

Make a hole here for rod wiring.

Take off original lock.

1.Original handle signal connector.

2.GND.

3.Suction lock connector.

4.Lock connector.

1.Front button

2.Batttery supply from insrance box.

3.CAN protocol position.

Make a hole for general front button.

Battery supply from this insurance box.

Battery and ACC.

Take off this 3 screws at the below of swc.

Here also has a screw.

Unplug this connector, plug to our special signal connector.

Lock and rear button.

Red arrow is for power/CAN/front button wiring diagram.

Blue arrow is for rod wiring diagram.

Yellow arrow is for kick sensor, if not have this function, no need install.

Press 3 times of unlock button on remote to open and close trunk.

After installation, power on and close the tail door manually, test the product to check whether the pole is pressed or not, the ball head gasket can be fine-tuned, if all working good, you can use our development center magic sticker and tie to fix control box and wiring, install each parts as where they are, the installation is complete!