GUIDE TECHNOLOGY(HK) LIMITED

INSTALLATION MANUAL

Car Model: YL-6241X 6267X HAVAL M6 M6 PLUS 2017+

Installation Requirement Safety Precautions

For your safety and normal using, please ask a professional personal to install it, do not install and uninstall by yourself, to avoid product damage or accidents.

Before installation, please make sure car mfd showing normally, all buttons inside car are working correctly, check if car light working, if have some scratches inside car surface, if yes, please contact with car owner.

Check if tailgate open and close normally, if has any deformations.

Prepare all tools, turn off car, ensure power off operation.

5.The parts and screws of the original car removed during installation should be placed separately and marked to prevent loss. Wire joints should be insulated to prevent short circuit.

6.According to the wiring mode of our company, avoid affecting the moving parts of the car when installation, such as steering wheel drive shaft, accelerator and brake pedal and other vehicle control parts. The wiring harness should be fixed during the straight line process to prevent loose.

7.Do not plug in or out the product and plug in the power-on state, to avoid damage to the product.

Step1: Wirring definition.

Pole serial no. seventh-bottom “L” means left pole, “R” means right pole, “G” means no need recognize.

Installation process diagram

Note: The installation step is to install the mechanical part of the pole firstly, open and close tailgate manually, and confirm that the polo open and close smoothly and the polo body does not scratch the car body, then connect the power and signal, then test again, if not problem, we can finish wiring followed our installation requirements.

Connect control box.

Rear button connector.

Connect our 3-ways connector.

Connect our suction lock(green color unlock signal, orange second lock signal).

Connect our power cable white color, its for kick sensor.

Kick sensor signal connector. Without kick sensor no need connect.

Kick sensor connector. Without kick sensor no need connect.

Control box power connector.

Battery.

ACC.

GND.

Second lock signal.

Rear button signal.

Rear button light.

Reserved.

CAN-L.

Unlock signal.

Rear button GND.

B-pillar unlock signal.

Manual signal.

CAN-H.

Above positions are the wiring diagrams of some models.

NOTE：After installed pole and lock, please open and close door manually to make sure it working perfectly without any scrub, then connect cable and testing with power on again, if working perfect, then we can begin to make wiring.

After the power is turned on, manually close the tailgate and reset it once, and test the machine to check whether the pole is pressed; the control box and various components are fixed with Velcro and cable ties provided by our development center. After several normal test runs, the original Reinstall all the plates of the car according to their original positions, and the installation is completed!